**Instalment #1**

**Quilt Block Name:**  Lady of the Lake



**Block Unfinished Size:**  12½"

**Number of Blocks to Make:**  Four

**Cutting Instructions:**


|  |  |  |  |
| --- | --- | --- | --- |
| **Colour** | **# to Cut** | **Size & Shape** | **Second Cut\*** |
| Colour A (Green) | 40 | 2⅞" Squares | http://www.blockcentral.com/images/hst.gif |
| Colour A (Green) | 2 | 8⅞" Square | http://www.blockcentral.com/images/hst.gif |
| Colour B (Cream) | 40 | 2⅞" Squares | http://www.blockcentral.com/images/hst.gif |
| Colour B (Cream) | 2 | 8⅞" Square | http://www.blockcentral.com/images/hst.gif |

\* http://www.blockcentral.com/images/hst.gif - *Cut once diagonally.* http://www.blockcentral.com/images/qst.gif - *Cut twice diagonally.*


**Sewing Instructions:**

***(Note:  Sewing Instructions are for 1 block.  You will need to make 4 identical blocks.)***


**Step 1:**  Place a Colour B (cream) 2⅞" triangle on a Colour A (green) triangle, right sides together.  Sew along the longest edge using a ¼" seam allowance.  Press the seam allowance toward the Colour A (green) fabric and trim points.  Make 20.  (Each unit should measure 2½".)



**Step 2:**  Place a Colour B (cream) 8⅞" triangle on a Colour A (green) triangle, right sides together.  Sew along the longest edge using a ¼" seam allowance.  Press the seam allowance toward the Colour A (green) fabric and trim points.  Make 1.  (This unit should measure 8½".)




**Step 3:**  Arrange four Step 1 units, as shown below.  Sew together using a ¼” seam allowance.  Press the seam allowances to one side.  Make 2.  (Each unit should measure 2½" x 8½".)




**Step 4.**  Arrange six Step 1 units, as shown below.  Sew together using a ¼" seam allowance.


Press the seam allowances to one side.  Make 2.  (Each unit should measure 2½" x 12½".)



**Step 5:**  Sew a Step 3 unit to the left side of the Step 2 unit.  Sew the remaining Step 3 unit to the right side of the Step 2 unit.  Press the seam allowances toward the Step 2 unit.  Make 1.  (This unit should measure 8½" x 12½".)



**Step 6:**  Sew a Step 4 unit to the top of the Step 5 unit.  Sew the remaining Step 4 unit to the bottom of the Step 5 unit.  Press the seam allowances toward the Step 5 unit.  Make 1.  (Your block will measure 12½" unfinished.  It will measure 12" when it is sewn into a quilt.)



**That's it!  Don't forget to make three more "Ladies" for a total of FOUR blocks!**